**SECTION 122413 - ROLLER WINDOW SHADES**

**PART I - GENERAL**

1.1 SCOPE

A. Manually operated roller shades with single rollers.

B .Related Requirements:

1.Section 061000 "Rough Carpentry" for wood blocking and grounds for mounting roller shades and accessories.

2.Section 079200 "Joint Sealants" for sealing the perimeters of installation accessories for light-blocking shades with a

sealant.

1.2 ACTION SUBMITTALS

A. Product Data: Include construction details, material descriptions, dimensions of individual components and profiles, features,

finishes, operating equipment, and instructions for roller shades.

B. Shop Drawings: Show fabrication and installation details for roller shades, including shadeband materials, their orientation to

rollers, and their seam and batten locations.

C. Samples for Verification: For each type of roller shade.

1. Shadeband Material: Not less than 10 inches square. Mark interior face of material if applicable.

2. Roller Shade: Full-size operating unit, not less than 16 inches wide by 36 inches long for each type of roller shade

indicated.

3. Installation Accessories: Full-size unit, not less than 10 inches long.

1.3 CLOSEOUT SUBMITTALS

A. Operation and Maintenance Data: For roller shades to include in maintenance manuals.

B. Warranty: For manufacturer's executed warranty documentation.

1.4 QUALITY ASSURANCE

A. Installer Qualifications: Fabricator of products.

B. Mockups: Build mockups to verify selections made under Sample submittals, to demonstrate aesthetic effects, and to set

quality standards for fabrication and installation.

1.5 DELIVERY, STORAGE, AND HANDLING

A. Deliver roller shades in factory packages, marked with manufacturer, product name, and location of installation using same

designations indicated on Drawings.

1.6 FIELD CONDITIONS

A. Environmental Limitations: Do not install roller shades until construction and finish work in spaces, including painting, is

complete and dry and ambient temperature and humidity conditions are maintained at the levels indicated for Project when

occupied for its intended use.

B. Field Measurements: Where roller shades are indicated to fit to other construction, verify dimensions of other construction

by field measurements before fabrication and indicate measurements on Shop Drawings. Allow clearances for operating

hardware of operable glazed units through entire operating range. Notify Architect of installation conditions that vary from

Drawings. Coordinate fabrication schedule with construction progress to avoid delaying the Work.

1.8 WARRANTY

A. Special Warranty for Shade Systems: Manufacturer agrees to repair or replace shade units that are not free from defects in

material or workmanship under normal and proper use within specified full warranty period, not prorated.

1.Warranty Period: Five years from date of Substantial Completion.

PART 2 – PRODUCTS

2.1 MANUFACTURERS

A. Source Limitations: Obtain roller shades from single source from single manufacturer. **Shades By Matiss/ 1148 US 22 Mountainside NJ 07092 Phone: 800-493-2040 Fax: 800-414-1042 / Website: www.shadesbymatiss.com**

2.2 **MANUALLY OPERATED SHADES WITH SINGLE ROLLERS**

A. Basis-of-Design Product: Subject to compliance with requirements, provide **Shades by Matiss Skyline Dual System**

B. Chain-and-Clutch Operating Mechanisms: With continuous-loop bead chain and clutch that stops shade movement when

bead chain is released; permanently adjusted and lubricated.

1. Bead Chains: Stainless Steel.

2. Loop Length: As indicated on Drawings

3. Limit Stops: Provide upper and lower ball stops.

4. Chain-Retainer Type: Chain tensioner, jamb mounted

C. Spring Lift-Assist Mechanisms: Manufacturer's standard for balancing roller shade weight and for lifting heavy roller shades.

1. Provide for shadebands that weigh more than 10 LB.

D. Rollers: Corrosion-resistant steel or extruded-aluminum tubes of diameters and wall thicknesses required to accommodate

operating mechanisms and weights and widths of shadebands indicated without deflection. Provide with permanently

lubricated drive-end assemblies and idle-end assemblies designed to facilitate removal of shadebands for service.

2. Roller Drive-End Location: As indicated on Drawings

3. Direction of Shadeband Roll: Regular, from back (exterior face) of roller

4. Shadeband-to-Roller Attachment: Manufacturer's standard method

E. Mounting Hardware: Brackets or endcaps, corrosion resistant and compatible with roller assembly, operating mechanism,

installation accessories, and mounting location and conditions indicated.

F. Shadebands:

1. Shadeband Material: Light-blocking fabric Sierra Sol Mesa, color as selected by Architect from manufacturer's full range

2. Shadeband Bottom (Hem) Bar: Exposed D30 with brush, color as selected by Architect from manufacturer's full range

G. Installation Accessories:

1. Front Fascia: Aluminum extrusion that conceals front and underside of roller and operating mechanism and attaches to

roller endcaps without exposed fasteners.

a. Shape: L-shaped.

b. Height: Manufacturer's standard height required to conceal roller and shadeband assembly when shade is fully open, but

not less than 5” inches

c. Side Channels: With light seals and designed to eliminate light gaps at sides of shades as shades are drawn down.

1. Installation Accessories, Edge Side Channels

2. Color As selected by Architect from manufacturer's full range

2.2 SHADEBAND MATERIALS

A. Shadeband Material Flame-Resistance Rating: Comply with NFPA 701. Testing by a qualified testing agency. Identify products

with appropriate markings of applicable testing agency.

B. Light-Blocking Fabric: Opaque fabric, stain and fade resistant.

1. Source: Shades by Matiss Sierra Sol Mesa

2. Type:  100% polyester with acrylic foam backing (PVC free)

3. Openness factor: Opaque

4. Thickness: 0.022 in

5. Weight: 9.4 oz/sq.yd

6. Orientation on Shadeband: As indicated on drawings

7. Color:  As selected by Architect from manufacturer's full range

8. Features: Fire-retardant

9. Outside face of light-blocking fabrics are often white.

2.3 ROLLER SHADE FABRICATION

A. Product Safety Standard: Fabricate roller shades to comply with WCMA A 100.1, including requirements for flexible, chain-loop

devices; lead content of components; and warning labels.

**PART 3 - EXECUTION**

3.1 EXAMINATION

A. Examine substrates, areas, and conditions, with Installer present, for compliance with requirements for installation tolerances,

operational clearances, and other conditions affecting performance of the Work.

B. Proceed with installation only after unsatisfactory conditions have been corrected.

3.2 ROLLER SHADE INSTALLATION

A. Install roller shades level, plumb, and aligned with adjacent units according to manufacturer's written instructions.

1.Opaque Shadebands: Located so shadeband is not closer than 2 inches to interior face of glass. Allow clearances for window

operation hardware.

B. Roller Shade Locations:  As indicated on Drawings

3.3 ADJUSTING

A. Adjust and balance roller shades to operate smoothly, easily, safely, and free from binding or malfunction throughout entire

operational range.

3.4 CLEANING AND PROTECTION

A. Clean roller shade surfaces, after installation, according to manufacturer's written instructions.

B. Provide final protection and maintain conditions, in a manner acceptable to manufacturer and Installer, that ensure that roller

shades are without damage or deterioration at time of Substantial Completion.

C. Replace damaged roller shades that cannot be repaired, in a manner approved by Architect, before time of Substantial

Completion.

3. DEMONSTRATION

A. Engage a factory-authorized service representative to train Owner's maintenance personnel to adjust, operate, and maintain

motor-operated roller shades.

**END OF SECTION 122413**